{"text_format":"2","workbook":"xls","n_sheets":6,"sheets":["Fahrzeugdaten","Reifen","Fahrwiderstand","Leistung","Leistungsdiagramm","Getriebe"],"not_rendered":{"charts":3,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Leistungsdiagramm","index":4,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Fahrzeugdaten","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
["Übersetzungen:"]
[null,"1. Gang","2. Gang","3. Gang","4. Gang","5. Gang","R. Gang","Achsübersetzung"]
["Getriebe XYZ",4.11,2.33,1.476,1.023,0.816,3.67,4.86]
["Getriebe ZXY",5.25,2.75,1.68,1.25,1,4.57,3.7857142857142856]
[]
[]
["Gewählt",5.25,2.75,1.68,1.25,1,4.57,3.7857142857142856]
[]
["Gesamtübersetzung",19.875,10.410714285714285,6.359999999999999,4.732142857142857,3.7857142857142856,17.300714285714285]
[]
[]
["Model","cw Wert","Stirnfläche A","cw * A","Gewicht des Fahrzeuges im Betrieb"]
["Einheit",null,"m²",null,"Kg"]
["vw lt Sven Hedin",0.45,5.02,2.259,3000]
["Auto XYZ"]
["Model Gewählt",null,null,2.259,3000]
[]
[]
["Schaltdrehzahl",3800]
[]
["Wirkungsgrad Antriebstrang",0.98]
[]
["p Luft",1.22,"kg/m³"]

{"sheet":"Reifen","index":1,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Reifen 185 R14"]
["Breite ",185,"mm"]
["Höhe/Breite",80,"%"]
["Felgendurchmesser",14,"Zoll"]
["rdyn @60km/h",0.3271032,"m"]
["rstat",0.3258,"m"]
["kr0",0.0135]
["kr1",0.0015]

{"sheet":"Fahrwiderstand","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["v","kr","Fa","P"]
["km/h",null,null,"kw"]
[10,0.01365,412.35213888888893,1.1454226080246914]
[20,0.0138,448.6645555555556,2.492580864197531]
[30,0.01395,506.24225000000007,4.218685416666667]
[40,0.0141,585.0852222222222,6.500946913580247]
[50,0.01425,685.1934722222222,9.51657600308642]
[60,0.0144,806.567,13.442783333333335]
[70,0.01455,949.2058055555555,18.456779552469133]
[80,0.0147,1113.109888888889,24.735775308641976]
[90,0.01485,1298.27925,32.45698125]
[100,0.015,1504.713888888889,41.797608024691364]
[110,0.01515,1732.4138055555554,52.93486628086419]
[120,0.0153,1981.3790000000001,66.04596666666667]
[130,0.01545,2251.6094722222215,81.30811983024688]
[140,0.0156,2543.105222222222,98.89853641975307]
[150,0.01575,2855.8662499999996,118.99442708333332]
[160,0.0159,3189.892555555555,141.77300246913578]
[170,0.016050000000000002,3545.184138888889,167.41147322530864]
[180,0.0162,3921.7409999999995,196.08704999999998]
[190,0.01635,4319.563138888889,227.976943441358]
[200,0.0165,4738.650555555556,263.2583641975309]

{"sheet":"Leistung","index":3,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Leistung P für MBK JX","Drehzahl","1. Gang","2. Gang","3. Gang","4. Gang","5. Gang","R. Gang"]
["Nm","1/min","vrad in km/h","vrad in km/h","vrad in km/h","vrad in km/h","vrad in km/h","vrad in km/h"]
[9,1000,6.203357894037736,11.842774161344767,19.385493418867924,26.05410315495849,32.56762894369811,7.126395830130878]
[14,1500,9.305036841056603,17.764161242017153,29.07824012830189,39.08115473243774,48.85144341554717,10.689593745196317]
[17,1750,10.855876314566038,20.724854782353344,33.924613483018874,45.59468052117736,56.9933506514717,12.471192702729036]
[21,2000,12.406715788075472,23.685548322689534,38.77098683773585,52.10820630991698,65.13525788739622,14.252791660261757]
[24.5,2250,13.957555261584904,26.64624186302573,43.61736019245283,58.6217320986566,73.27716512332077,16.034390617794475]
[27,2500,15.508394735094337,29.606935403361923,48.46373354716981,65.13525788739622,81.41907235924529,17.815989575327194]
[29,2750,17.059234208603772,32.56762894369811,53.3101069018868,71.64878367613585,89.56097959516981,19.597588532859913]
[32,2900,17.98973789270943,34.34404506789982,56.21793091471698,75.55689914937963,94.44612393672452,20.666547907379545]
[36.4,3000,18.610073682113207,35.528322484034305,58.15648025660378,78.16230946487548,97.70288683109435,21.379187490392635]
[39.8,3100,19.230409471516978,36.71259990016878,60.09502959849058,80.76771978037134,100.95964972546416,22.09182707340572]
[42.1,3200,19.850745260920753,37.89687731630326,62.03357894037736,83.37313009586718,104.21641261983397,22.80446665641881]
[43.6,3300,20.471081050324525,39.08115473243773,63.972128282264144,85.97854041136301,107.47317551420377,23.517106239431893]
[44.5,3400,21.0914168397283,40.26543214857221,65.91067762415095,88.58395072685887,110.72993840857359,24.229745822444983]
[45,3500,21.711752629132075,41.44970956470669,67.84922696603775,91.18936104235472,113.9867013029434,24.942385405458072]
[45.4,3600,22.332088418535847,42.633986980841165,69.78777630792453,93.79477135785056,117.24346419731323,25.65502498847116]
[45.9,3700,22.95242420793962,43.81826439697564,71.72632564981133,96.40018167334642,120.50022709168303,26.36766457148425]
[46.5,3800,23.572759997343393,45.00254181311011,73.66487499169811,99.00559198884226,123.75698998605284,27.080304154497334]
[47.2,3900,24.19309578674717,46.18681922924459,75.60342433358491,101.6110023043381,127.01375288042264,27.792943737510424]
[47.9,4000,24.813431576150943,47.37109664537907,77.5419736754717,104.21641261983396,130.27051577479244,28.505583320523513]
[48.5,4100,25.43376736555472,48.55537406151355,79.4805230173585,106.82182293532982,133.52727866916229,29.218222903536596]
[48.9,4200,26.05410315495849,49.73965147764803,81.41907235924529,109.42723325082568,136.7840415635321,29.930862486549685]
[49.4,4300,26.67443894436226,50.923928893782495,83.35762170113208,112.03264356632151,140.04080445790188,30.643502069562775]
[49.8,4400,27.294774733766033,52.10820630991698,85.29617104301886,114.63805388181736,143.2975673522717,31.35614165257586]
[50.3,4500,27.91511052316981,53.29248372605146,87.23472038490566,117.2434641973132,146.55433024664154,32.06878123558895]
[50.7,4600,28.535446312573583,54.47676114218593,89.17326972679246,119.84887451280906,149.81109314101133,32.78142081860204]
[50.9,4700,29.15578210197736,55.66103855832041,91.11181906867925,122.45428482830492,153.06785603538114,33.49406040161513]
[50.2,4800,29.77611789138113,56.845315974454884,93.05036841056602,125.05969514380075,156.32461892975095,34.206699984628216]

{"sheet":"Getriebe","index":5,"n_rows":7,"n_cols":21,"rows_kept":7,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[{"$nulls":16},"Schaltdrehzahl:"]
[{"$nulls":16},3800]
[{"$nulls":17},"Schaltvorgang:"]
[{"$nulls":17},"1. - 2. Gang","2. - 3.Gang","3. - 4. Gang","4. - 5. Gang"]
[{"$nulls":16},"n nach Schalten [1/min]",1990.4761904761904,2321.4545454545455,2827.3809523809523,3039.9999999999995]
[{"$nulls":16},"V in [km/h]",23.572759997343393,45.00254181311011,73.66487499169811,99.00559198884226]